(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "top_cu")
		(2 "B.Cu" signal "bottom_cu")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_00000000_000000af)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(P3-P1)")
	(net 3 "Net-(P2-P1)")
	(net 4 "Net-(U1A-K)")
	(net 5 "Net-(P1-PM)")
	(net 6 "Net-(P4-P1)")
	(net 7 "Net-(P4-PM)")
	(net 8 "unconnected-(P5-Pad1)")
	(net 9 "unconnected-(P6-Pad1)")
	(net 10 "unconnected-(P7-Pad1)")
	(net 11 "unconnected-(P8-Pad1)")
	(net 12 "Net-(U1A-G)")
	(net 13 "Net-(U1B-K)")
	(footprint "Footprints:CP_Radial_D10.0mm_P5.00mm"
		(layer "F.Cu")
		(at 141.605 99.695 90)
		(descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at 4.953 -5.969 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 2.5 6.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(P3-P1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:C_Disc_D4.7mm_W2.5mm_P5.00mm"
		(layer "F.Cu")
		(at 137.16 125.095 90)
		(descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=4.7*2.5mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 5.00mm  diameter 4.7mm width 2.5mm Capacitor")
		(property "Reference" "C2"
			(at 2.5 -2.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "680nF"
			(at 2.5 2.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C? C_????_* C_???? SMD*_c Capacitor*")
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(P2-P1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U1A-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.7mm_W2.5mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 125.095 93.98)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "P5"
			(at 4.505 -1.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "MOUNTING_HOLE"
			(at 2.905 2.52 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(P5-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Footprints:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 169.545 93.98)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "P6"
			(at -3.945 -1.98 180)
			(layer "F.SilkS")
		)
		(property "Value" "MOUNTING_HOLE"
			(at -2.745 2.52 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(P6-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Footprints:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 169.545 132.715)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "P7"
			(at 0 -3.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "MOUNTING_HOLE"
			(at -6.245 2.285 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(P7-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 136.271 107.95 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 0.381 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "1.5K"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(U1A-G)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U1A-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 156.21 95.885 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "1.5K"
			(at 3.81 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(U1B-K)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 164.465 117.475 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "47K"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(P1-PM)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:Altech_AK300_1x02_P5.00mm_45-Degree"
		(layer "F.Cu")
		(at 128.27 112.776 -90)
		(descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
		(tags "Altech AK300 serie connector")
		(property "Reference" "P2"
			(at 8.724 1.67 0)
			(layer "F.SilkS")
		)
		(property "Value" "OUT"
			(at 2.5 7.5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.7 2.75 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(P2-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "PM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:Altech_AK300_1x02_P5.00mm_45-Degree"
		(layer "F.Cu")
		(at 128.27 100.711 -90)
		(descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
		(tags "Altech AK300 serie connector")
		(property "Reference" "P3"
			(at 2.489 -7.43 270)
			(layer "F.SilkS")
		)
		(property "Value" "POWER"
			(at 2.5 7.5 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.7 2.75 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(P3-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "PM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:Altech_AK300_1x02_P5.00mm_45-Degree"
		(layer "F.Cu")
		(at 145.542 131.191)
		(descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
		(tags "Altech AK300 serie connector")
		(property "Reference" "P4"
			(at -4.342 -1.291 0)
			(layer "F.SilkS")
		)
		(property "Value" "CONN_2"
			(at 2.5 7.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.7 2.75 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(P4-P1)")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(P4-PM)")
			(pinfunction "PM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 133.985 125.095 180)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "100K"
			(at 3.81 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_* Resistor_*")
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(P2-P1)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:Valve_ECC-83-1"
		(layer "F.Cu")
		(at 149.225 113.665)
		(descr "Valve ECC-83-1 round pins")
		(tags "Valve ECC-83-1 round pins")
		(property "Reference" "U1"
			(at 12.7 -1.397 0)
			(layer "F.SilkS")
		)
		(property "Value" "ECC83"
			(at -3.45 6.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.05 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 3.45 4.8)
			(size 2.03 2.03)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(U1A-G)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.6 1.87)
			(size 2.03 2.03)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(P1-PM)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.6 -1.78)
			(size 2.03 2.03)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(U1B-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 3.45 -4.71)
			(size 2.03 2.03)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(P4-PM)")
			(pinfunction "F1")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 -5.85)
			(size 2.03 2.03)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(P4-PM)")
			(pinfunction "F1")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at -3.46 -4.71)
			(size 2.03 2.03)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(P3-P1)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at -5.61 -1.78)
			(size 2.03 2.03)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(U1A-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at -5.61 1.83)
			(size 2.03 2.03)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U1A-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at -3.46 4.8)
			(size 2.03 2.03)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(P4-P1)")
			(pinfunction "F2")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3d_shapes/ecc83.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:Altech_AK300_1x02_P5.00mm_45-Degree"
		(layer "F.Cu")
		(at 166.37 105.41 90)
		(descr "Altech AK300 serie terminal block (Script generated with StandardBox.py) (http://www.altechcorp.com/PDFS/PCBMETRC.PDF)")
		(tags "Altech AK300 serie connector")
		(property "Reference" "P1"
			(at 0 -7.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "IN"
			(at 2.5 7.5 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.7 2.75 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "P1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(P1-PM)")
			(pinfunction "PM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/TerminalBlock_Altech.3dshapes/Altech_AK300_1x02_P5.00mm_45-Degree.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Footprints:MountingHole_3.2mm_M3_DIN965_Pad"
		(layer "F.Cu")
		(at 125.095 132.715)
		(descr "Mounting Hole 3.2mm, M3, DIN965")
		(tags "mounting hole 3.2mm m3 din965")
		(property "Reference" "P8"
			(at 0 -3.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "MOUNTING_HOLE"
			(at 0 3.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Racine")
		(sheetfile "ecc83-pp.kicad_sch")
		(attr through_hole exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.6 5.6)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(P8-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 173.355 90.17)
		(end 173.355 136.525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.285 90.17)
		(end 121.285 136.525)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.355 90.17)
		(end 121.285 90.17)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.285 136.525)
		(end 173.355 136.525)
		(layer "Edge.Cuts")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.635)
		)
		(min_thickness 0.381)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.50038)
		)
		(polygon
			(pts
				(xy 172.085 135.89) (xy 172.085 91.313) (xy 122.555 91.44) (xy 122.555 135.89)
			)
		)
	)
	(embedded_fonts no)
)
